NulMrx

This is a simple network provider and driver provided to illustrate how network providers bind to the Multi-Protocol Router and redirectors to the Multiple UNC Provider. The nulmrx sample has very limited functionality:

1. Map a share like net use * \\nulsvr\share.

2. Enumerate the directory on the drive mapped above and see the volume info and a sample file at the root.

This is all faked in the driver code. It has no create/read/write abilty.

Installation:

1. Run regini nulmrx\sys\nulmrx.ini
2. Edit the following registry entry to add NulMRx as the first network provider: \\HKEY_LOCAL_MACHINE\System\CurrentControlSet\Control\NetworkProvider\Order\ProviderOrder REG_SZ NulMRx, LanmanWorkstation
3. Reboot to let the nulmrx driver register with the system.