The remote redirector samples come in the form of two sets of file system components: nulmrx and smbmrx

SMBMrx

The smbmrx is a fully functional network provider, with the ability to communicate with any server that supports NT4 level of CIFS, including working with a domain or workgroup server.

Installation:

1. Run smbmrx\exe\*\smbrdr.exe.
2. Click on the “Provider” button and move SMBMRx above the LanmanWorkstation provider in the network provider order.
3. Click on “Load” to install and load the necessary components.
4. Click “Start” to start the redirector driver.
5. Now you can run any standard net command and communicate with any CIFS server that supports the NT4 dialect.